## Summary

This processor listens to SNMP traps and creates a flowfile from the trap PDU. The versions SNMPv1, SNMPv2c and SNMPv3 are supported. The component is based on SNMP4J.

SNMPv3 has user-based security. The USM Users Source property allows users to choose between three different ways to provide the USM user database. An example json file containing two users:

    [
       {
          "securityName":"user1",
          "authProtocol":"MD5",
          "authPassphrase":"abc12345",
          "privProtocol":"DES",
          "privPassphrase":"abc12345"
       },
       {
          "securityName":"newUser2",
          "authProtocol":"MD5",
          "authPassphrase":"abc12345",
          "privProtocol":"AES256",
          "privPassphrase":"abc12345"
       }
    ]